ROACH 2 Manufacturing Pack

The manufacturing pack consists of 4 folders:

dcoumentation – Drawings and Information

dxf – Autocad 2d files

silkscreens – Silkscreens for the front panel, back panels and back

stp\_files – 3D Step Files

A single ROACH 2 Enclosure consists of:

1 x ROACH 2 CHASSIS

1 x ROACH 2 LID

1 x FRONT PANEL

2 X BACK PANEL, blanks by default

The entire chassis is made of Aluminium with a Kenverted finish, except the FRONT PANEL which has a brushed anodised finish.