ROACH 2 Manufacturing Pack

The manufacturing pack consists of x folders

A single ROACH 2 Enclosure consists of:

1 x ROACH 2 CHASSIS

1 x ROACH 2 LID

1 x FRONT PANEL

X BACK PANEL

The entire chassis is made of Aluminium with a Kenverted finish, except the FRONT PANEL which has a brushed anodised finished